s_WaitForTimer

s_DACWrite

DACEnable = 0 D=outputdata timerClk = 1

s_ADCEnable

/ADCEnable = 0 ADCRead = 0 ConvolverStart = 1 ConvolverStartAddr = addr - 1

3 clock cycles

s_ADCWait

/ADCEnable = 0 ADCRead = 1

ADCStatus = 1 and ConvolverBusy = 1

s_ADCRead

/ADCEnable = 0 ADCAead = 1 inputdata = D outputdata = ConvolverResult

ADCStatus = 0 and ConvolverBusy = 0

s_RAMWrite

RAMWE = 1 RAMAddr = addr RAMData = inputdata addr = addr + 1