s_Idle

i = -1 BaseAddr = StartAddr

s_AddrSelect

busy = 1 i = i + 1 RamAddr = BaseAddr - i - 1 RomAddr = i + 1 accumulator = accumulator + MultResult start = 1

s_StartMult

busy = 1 RamAddr = BaseAddr - i - 1 RomAddr = i + 1 MultStart = 1

s_WaitMult

busy = 1 RamAddr = BaseAddr - i - 1 RomAddr = i + 1

MultBusy = 1

MultBusy = 0 and i < 15

s_Output

result = accumulator[14..7]

MultBusy = 0 and i = 15